Annex No. 2
Technical Specification
The Equipment consist of 64 identical power supply units. Each unit must meet the technical conditions listed in this table.
	No.
	Description and minimum specification of the Equipment as defined by the Contracting Authority
	Description and specification of the Equipment offered by the Bidder
	Complies YES/NO

	1
	Programmable PSU
	
	

	2
	Single-phase input voltage: 230 VAC
	
	

	3
	Output voltage: 0-300 VDC
	
	

	4
	Output current: 0-9 A
	
	

	5
	Power: max. 2700 W
	
	

	6
	Frame: 19" Rack - 1U
	
	

	7
	Control and monitoring via LAN / USB / RS232 / RS485 & Analog
	
	

	8
	Isolated signal converter 0-5V / 0-10V
	
	

	9
	Compatibility with CERN-customized LabVIEW controlling SW
	
	



(Bidder shall fill in the columns “Description and specification of the Equipment offered by the Bidder” and “Complies YES / NO”)

