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Annex No. 1 to the Contract
 
Technical Specification of the Supply
Technical parameters table of fog and cloud droplet monitor

	Parameter
	Required value
	Offered value to be delivered

	Mode of operation
	Long-term, continuous
Remote control possible
Remote access to data
	

	Sampling head
	With heating
	

	Particle size range
	0.6 – 40 µm
	

	Number of size bins
	min. 30
	

	Range of particle number concentration
	0 – 1000 # / cm3
	

	Power consumption
	max. 600 W
	

	Ambient temperature during operation
	-30 ºC - +50ºC
	

	Weight
	max. 40 kg
	

	Output data
	Particle size distribution
Particle number concentration
Median volume diameter
Effective diameter
Liquid water content
	

	Output data rate
	Selectable
	



