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4b) Tabulka parametrů zboží určeného k plnění zakázky
HARDWARE PRO LOKÁLNÍ SBĚR DAT
(tabulka může být vyplněna v anglickém jazyce)
	Položka
	Zadavatelem požadovaná hodnota
	Uchazečem nabízená hodnota zboží určeného 
k plnění
	Obchodní název dodávaného zboží

	Processor
	2xCPU with benchmark at minimum 13 500 points: http://www.cpubenchmark.net/multi_cpu.html
Hardware virtualization support
	
	

	RAM
	Minimum 128 GB DDR3 ECC
Minimum 1600MHz frequency
Support for up to 1TB ECC RAM
	
	

	Storage interfaces
	Support at minimum 2xSATA 3.0 6Gb/s AHCI, RAID 0,1,5,10
Support at minimum 2xSATA 2.0 3 Gb/s AHCI, RAID 0,1,5,10
Support at minimum 2xSATA 2.0 3 Gb/s SCU, RAID 0,1,5,10
	
	

	Disk
	At minimum 1TB  net disk space SATA 3.0, 7200rpm
	
	

	DVD
	48x DVD ROM or RW
	
	

	Connectivity
	At minimum 2x 1Gb ethernet RJ 45, support for 10/100/1000BASE-T

At minimum 4x 10Gb/s ethernet, 4x SFP+ slots, card in one PCIe x8 slot. Card must support: PCIe x3.0, RDMA (Remote DMA), TOE (TCP Offload Engine), jumbo frames,  VMDq and PC-SIG SR-IOV foLarge receive offload (LRO), Linux.r Virtualized Environments,  iSCSI remote Boot,  PXE boot, Large send offload (LSO), Large receive offload (LRO), RSS (Receive Side Scaling), Linux.
	
	

	Expansion slots
	PCIe 3.0
At minimum 6x PCIe 3.0 x8 (or x16) signal lines
At maximum 11x PCIe 3.0 x8 (or x16) signal lines.
All devices in PCIe slots must be accessible from front doors when mounted in rack. Standard height in all slots must be supported.
All slots must support full length cards. All cards must be mounted vertically.
	
	

	USB
	At minimum 8x USB 2.0 or 3.0.
At minimum 4 USB ports accessible from front doors when mounted in rack.
	
	

	Video
	1x VGA video accessible from front panel
	
	

	Management support
	Support for IPMI 2.0 on dedicated RJ45 ethernet port
	
	

	OS compatibility
	Linux X86 64bit, RedHat, SuSe
	
	

	Electric connection
	European slot
	
	

	Chassis
	Rack mount 19”
Size  3 or 4 rack units (U)
Delivery must contain whole rack mount kit including sliding-rails.
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