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Technical parameters of the offer
Contracting authority: PILANA Metal s.r.o., IČO 25328956

Name of supplier: 
Delivery of a blasting machine for continuous blasting of bandsaw blades 

(to be completed by the supplier if bidding for sub-delivery 1)






       

	Material that can be processed in the offered machine
	Band width 12,7 - 80mm
	Yes - no

	
	Band thickness 0,6 - 1,6 mm
	Yes - no

	
	Body hardness 50HRC, tooth hardness 69 HRC
	Yes - no

	
	Coil length up to 303 m
	Yes - no

	Technical parameters of the offered machine
	Continuous passage of connected bands
	Yes - no

	
	Uniform band color over the entire width and length of the coil
	Yes - no

	
	Band is clean and dry at the exit
	Yes - no

	
	Integrated washing device has a closed water circuit
	Yes - no

	
	Increase in curvature in any part of the tooth profile by a maximum of 30µm compared to the initial condition
	Yes - no

	
	Equipment output for 34mm x1.1mm, ¾ TPI reference belt min 8 m/min
	Yes - no

	
	Dust content up to 5mg/m3
	Yes - no

	
	Possibility to control the amount of abrasive used
	Yes - no

	
	Automatic abrasive dosing
	Yes - no

	Total quoted tender price includes
	Blasting machine
	Yes - no

	
	Transportation, commissioning, operator training and all other related costs
	Yes - no

	Signature of the person authorised to act for the supplier:
	


Supply of unwinding and coiling equipment for feeding bandsaw blades 

(to be completed by the supplier if bidding for sub-delivery 2)
	Material that the offered device can coil and unwind
	Band width  13 - 80mm
	Yes - no

	
	Band thickness  0,5 - 1,6mm
	Yes - no

	
	Outer diameter of the coil 1000mm
	                 Yes - no

	Technical parameters of the offered machine

	Horizontal placement of coils
	Yes - no

	
	The bottom of the coil is at a height of 1000 mm from the floor with a regulation of at least +/- 50 mm
	Yes - no

	
	The band is clean and dry at the outlet
	Yes - no

	
	There is an automatic centre lock to hold the beginning of the saw blade
	Yes - no

	
	Continuously adjustable winding speed 0 - 10 m/min
	Yes - no

	
	The coiling speed is constant at the set level
	Yes - no

	
	Neither the unwinding nor the coiling device damages the tooth tips
	Yes - no

	Total quoted tender price 

includes
	1 pc unwinding device + 1 pc coiler
	Yes - no 

	
	Transportation to the place of delivery
	Yes - no

	Signature of the person authorised to act for the supplier:
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