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1. Identification of the contracting entity
	Name of the contracting entity
	PILANA Metal, s.r.o.

	ID number, Tax ID number of the contracting entity
	IČ 25328956; DIČ CZ25328956

	Contact address of the contracting entity
	Nádražní 804, 768 24  Hulín

	Person authorised to act for the contracting entity
	Ing. Lenka Straková, jednatelka

	Contact person for the contract
	Ing. Jiří Michal, jednatel

	Contracting entity profile/electronic tool
	https://www.e-zakazky.cz/profil-zadavatele/69d74dd9-65f2-4dc7-aadf-3c6cb808e983 


This tender is part of a project co-financed by the European Union under the National Recovery Plan - Circular Solutions in Enterprises Programme - Call I.

This tender procedure is announced in accordance with Act No. 134/2016 Coll., on public procurement, as amended, in the "Simplified sub-limit procedure". 
1. Subject of the contract
The subject of the contract is divided into two parts (hereinafter referred to as sub-delivery). 

A tenderer may submit an offer for one or both sub-deliveries. Each sub-delivery will be evaluated separately.
Sub-delivery 1: 

The subject of delivery is equipment for continuous blasting of bandsaw blades, in order to achieve the desired surface finish of bandsaw blades.
The machine must be able to process bands of the following characteristics:
Band width: 12.7 - 80 mm 

Band thickness: 0.6 - 1.6 mm 

Band material: hardened Bi-metal 

Hardness: teeth - 69 HRC; body 50 HRC  

Bands are coiled in rolls of up to 303 metres.
The machine must meet the following requirements: 

· Continuous passage of non-rigidly connected strips (end of coil + beginning of new coil are only taped together)

· After blasting, the colour is uniform over the entire width and length of the coil

· The band must be clean and dry at the exit, the integrated washing device must have a closed water circuit  

· The blasting process must not damage the tooth tips - the acceptable increase in curvature during blasting in any part of the tooth profile is a maximum of 30µm compared to the initial condition

· Required minimum machine performance for reference strip: 34mm x1.1mm, ¾ TPI strip; minimum 8m of blasted strip per minute required

· Dust content: max 5 mg per m3 

· Possibility to control the amount of abrasive used (decrease/increase blasting power), for example by switching additional nozzles on/off

· Automatic abrasive dosing
Classification of equipment according to NIPEZ: 42631000-8 Machining and forming machines for finishing of metals.
The tenderer's tender for sub-delivery 1 shall meet all the technical requirements specified. The tenderer shall declare compliance with these requirements by attaching to its tender the document Technical parameters of the tender, completed in the section 'Sub-delivery 1'. The Bid Specifications document form is attached as Annex 2 to this Tender Document.
Sub-delivery 2: 

The subject of delivery is equipment for unwinding (1pc) and coiling (1pc) of bandsaw blade coils.

The unwinding device unwinds the saw blades from the coil and feeds them into the machine. After the operation, the coiling device will coil the processed saw blades back onto the coil.
The unwinding and coiling device works with saw band coils. 

Band width: 13 - 80mm, band thickness 0,5 - 1,6mm.

The outer diameter of the coil is up to 1000mm. The coils are placed horizontally on the unwinding and coiling device. 

The coil must be placed at a specified height of 1000mm (measured from the floor) on the unwinding and coiling device with a minimum regulation of +/- 50mm:  
The unwinding and coiling device must be equipped with an automatic centre lock to hold the beginning of the saw band, which will then be coiled into the coil.

The coiler shall have a continuous speed regulation in the range 0-10 m/min, the coiling speed shall be constant at the set speed setting. 

The tooth tips must not be damaged during coiling /unwinding.
Classification of equipment according to NIPEZ: 42411000-0 Winches and jacks.
The tenderer's tender for sub-delivery 2 shall meet all the technical requirements specified. The tenderer shall declare compliance with these requirements by attaching to its tender the document 'Technical parameters of the tender', completed under 'Sub-delivery 2'. The Bid Specifications document form is attached as Annex 2 to this Tender Document.

The tenderer shall include in the tender price all components, works and services related to the delivery of the contract at the place of delivery (i.e. the full price of the equipment specified above, including transport to the place of delivery and commissioning by a qualified employee of the supplier). The contracting authority shall ensure that the machine is unloaded at the place of delivery, settled on site and connected to the power grid.
In the tender, the tenderer shall indicate the total price for the complete delivery, excluding VAT, in Czech crowns or in EUR.
2. Estimated value of the contract
The estimated value of sub-delivery 1 is EUR 186.000.

The estimated value of sub-delivery 2 is EUR 26 000.
3. Place and term of delivery
The place of delivery for both partial deliveries is the headquarters of the contracting authority at Hulín, Nádražní 804. No inspection of the place of delivery will take place.

The required delivery date is until 20.9.2024 (the deadline for the final handover of the functional machine without defects and imperfections to the contracting authority at the place of delivery). The contracting authority reserves the possibility of future changes to this condition (in accordance with §100 of the Public Procurement Act, any extension of the delivery date by a contract amendment will not be a material change to the contract obligation).
4. Proof of qualifications
The tenderer is obliged to prove the fulfilment of the qualification requirements within the tender submission. For this purpose, the tenderer shall attach to the bid:
- a completed affidavit of basic competence (Annex 4 of this Tender document)
- a plain copy of an extract from the commercial register or other similar register of business entities.
5. Method of processing the offer
The tender shall be prepared in Czech or English, in written form, signed by an authorised representative of the tenderer.

The tenderer may submit a tender for one or both sub-deliveries.
The offer will be structured as follows:

· Tender Cover Sheet (the form of the cover sheet is attached as Annex 1 to this tender documentation)

· Completed Tender Specifications Sheet (see Annex 2 to this tender documentation).

· The contract for the work to be completed by the tenderer with the prescribed information and signed by an authorised representative of the tenderer (see Annex 3 to this ToR)

· An affidavit of the basic competence of the tenderer (see Annex 4 to this ToR)

· Extract of the tenderer from the commercial register (or other register of entities authorised to do business) - a plain copy
6. Method of submission of tenders, deadline
The tender will be prepared in written form in accordance with the structure set out in Section 5 of this document. 

The entire tender will be scanned as a PDF document.

The tender must be submitted within the deadline for submission of tenders. The deadline for submission of tenders is 11 January 2024 at 09:00. 

Tenders may only be submitted electronically via the contracting authority's profile at e-zakazky.cz. A tenderer intending to submit a tender is obliged to register in the electronic tool. Submission of a tender is only possible after registration and login to the electronic tool.

The contracting authority does not accept variants (a tenderer may submit only one tender).

The contracting authority will open tenders after the deadline for the submission of tenders. Opening of a tender in electronic form means making its contents available to the contracting authority.

In view of the fact that the contracting authority allows, in accordance with Section 211(3) of the Public Procurement Act, the submission of tenders in electronic form, the opening of tenders will take place without the presence of the tenderers.
7. Criteria and evaluation of tenders
Tenders will not be evaluated if they do not meet the completeness requirements and do not contain all the information and documents that are required as part of the tender. The tenders will be opened, evaluated for compliance with the tender documentation and evaluated by an evaluation committee appointed by the contracting authority, and minutes of the opening, evaluation and assessment of the tenders will be taken. The evaluation will be carried out separately for each sub-performance. 

The sole evaluation criterion shall be the lowest tender price for both lots, which will determine the overall ranking of the tenderers. For each sub-performance, the tender with the lowest tender price shall be the successful tenderer.
8. Provision of additional information
The tenderer is entitled to ask the contracting authority for a written explanation of the terms of reference. 

A written request for an explanation of the tender documentation shall be submitted electronically in Czech or English via an electronic tool (the contracting authority's profile). 

The written request must reach the contracting authority at the latest 4 working days before the deadline for submission of tenders. The contracting authority may also provide an explanation of the tender specifications without a prior request or on the basis of a late request. 

The contracting authority shall publish the clarification of the specifications (without identifying the tenderer who requested the clarification), including the exact wording of the question, on the contracting authority's profile.

The contracting authority shall send the clarification of the specifications no later than 2 working days after receipt of the request. If the request for clarification of the specifications is received in time and the contracting authority does not publish, send or transmit the clarification within 2 working days, it shall extend the deadline for submission of tenders by at least as many working days as the time elapsed between the receipt of the request for clarification of the specifications and the publication, sending or transmission of the clarification.
9. Other conditions of the contracting authority
The contracting authority reserves the right to cancel the tender procedure under the terms of the ZZVZ.

The contracting authority does not grant the tenderer the right to reimbursement of costs associated with participation in the selection procedure.
The official document of the tender procedure is the tender documentation in the Czech language. This translation into English is an auxiliary document. In the event of a conflict of versions, the Czech version shall prevail.
10. Annexes
Annex 1: Tender Cover Sheet Form

Annex 2: Form Technical parameters of the offer

Annex 3: Contract for the work
Annex 4: Affidavit of the basic competence
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